===============================================================================

                           Microsoft Windows95 English

                         FUJITSU DL3750+ Printer Driver

                                  Version 3.40

                    Copyright(C) 2005 FUJITSU ISOTEC LIMITED
===============================================================================

This printer driver works on the following operating systems:

  Microsoft(R) Windows(R) 95 English (referred to as Windows95)

This printer driver is for FUJITSU DL3750+ printers.



Contents

1. Printer driver operating environment
2. Printer driver configuration
3. Printer driver setup
  3.1 Before setting up
  3.2 Setup from "New Hardware Found"
    3.2.1 for 4.00.950 or 4.00.950A
    3.2.2 for 4.00.950B or 4.00.950C
  3.3 Setup from "Add Printer"
4. Printer driver setup method
5. Others
- About the trademark

NOTE: This driver is for FUJITSU DL3750+ printers.
      Do not use it on other printers.
      When printing using Windows95, change the printer settings back to the
      factory default.
      Otherwise printer may not function as expected.



1. Printer driver operating environment

- Hardware
  PC's with the English-version Windows95

- Target operating system
  Windows95 (English-version)

NOTE:  This product only operates on English-version Windows95.



2. Printer driver configuration

  FUJITSU DL3750+ printer driver consists of the following files:

   DL3750.DRV    FUJITSU DL3750+ printer driver
   NRBMON.DLL    FUJITSU DL3750+ Language Monitor
   DL3750.INF    Setup information file
   README.TXT    This file



3. Printer driver setup

---------------------
3.1 Before setting up
---------------------
- Prepare the following for setup:
   1) Windows95 operating system          (CD-ROM)
   2) FUJITSU DL3750+ Printer Driver Disk (this disk)

- Set up FUJITSU DL3750+ from "New Hardware Found".
  If "New Hardware" is not found, set up from "Add Printer".

- If the FUJITSU DL3750+ printer driver has already been set up, delete
  it and set up again.


------------------------------------
3.2 Set up from "New Hardware Found"
------------------------------------
When setting up from "New Hardware Found", the screen may appear differently
depending on the version of Windows95 used.
Click the right button of the mouse on the "My computer" icon and select
"System properties" from "General".


3.2.1  for 4.00.950 or 4.00.950a
================================
a. Connect the printer to the PC and turn on the printer.

b. Turn on the PC, and start Windows95.  Restart Windows95 if it is already
   started.

c. When "New Hardware Found" dialogue appears, select "Driver from disk
   provided by hardware manufacturer", and click "OK".

d. Insert this printer setup disk in the CD drive.

e. Enter "D:\Drivers\DL3750+\English\Win95" (if the D: is the CD drive) into
   the "distributed file copy source", and click OK.
   NOTE: When the dialogue "insert disk" appears, click "OK", enter
         "D:\Drivers\DL3750+\English\Win95"(if the D: is the CD drive)
         into the "file copy source", and click OK.
         In addition, insert Windows95 system CD-ROM if required, and
         click "OK".  Enter "D:\WIN95 " into "file copy source" or click
         "reference" and select "D:\WIN95".

f. Follow the directions and continue with the setup.
   NOTE: If there is a conflict (if "there is a newer file than the one to be
         copied, and users are advised to use the already existing file"
         appears), click "yes".

g. Added printer icon appears in the "Printers" folder".

The printer driver setup is now complete.


3.2.2  for 4.00.950B or 4.00.950C:
==================================
a. Connect the printer to the PC and turn on the computer.

b. Turn on the PC, and start Windows95.  Restart Windows95 if it is already
   started.

c. When "Update Device Driver Wizard" appears, click "next".

d. Click "Other Locations...".

e. Insert the printer setup disk in the CD drive

f. Enter "D:\Drivers\DL3750+\English\Win95" (if the D: is the CD drive) as
   "Location", and click "OK".

g. When "Update Device Driver Wizard" appears, click "Finish".

h. Follow the instructions on the screen and continue with the setup.
   NOTE: When the dialogue "Insert Disk" appears, click "OK", enter
         "D:\Drivers\DL3750+\English\Win95" (if D: is the CD drive) for
         the "Copy files from:", and click "OK".
         The user may be required to insert the Windows95 system CD-ROM.
         Click "OK" after inserting the CD-ROM.  Enter "D:\WIN95" for the
         "Copy files from:" or click  "Browse" and select "D:\WIN95".

i. An icon of the added printer will appear in the "printer" folder.

Printer driver setup is now complete.



----------------------------
3.3 Setup from "Add Printer"
----------------------------
Start Add Printer Wizard.
The following is the FUJITSU DL3750+ setup procedure after Windows95
is started up.

a. Go to "Start" -> "Settings" ->"Printers".

b. Double-click "Add Printer".

c. The "Add Printer Wizard" will appear.
   Follow the instructions on the screen and proceed.

d. When the printer list from the manufacturer appears click on "Have Disk".

e. Insert the printer setup disk into the CD drive, enter "D:\Drivers\DL3750+
   \English\Win95" (if D: is the CD drive) as the "Copy manufacture's files
   from:", and click "OK".

f. The model names will be listed in the "Printers" list box.  Select the model
   and click  "next".
   NOTE: When the message "A driver is already installed for this printer.
         Would you like to keep the existing driver or use the new driver one?
         Your programs may print differently if you use the new driver",
         appears, select "Replace existing driver".

g. Select the "Available ports".

h. Confirm the printer name, and set it as the default printer, and click on
   "next".

i. Perform a printout test if desired, and select "next".
   NOTE: The user may be required to insert the Windows95 system CD-ROM.  Click
         "OK" after inserting the CD-ROM.  Enter "D:\WIN95" for the "Copy files
         from:" or click  "Browse" and select "D:\WIN95".

j. As in [i.], when "Print Test Page" is selected, a dialogue box will appear
   when printing is completed.  Click the "OK" or "No" button.
   Note with Test Page:
     - Printing will proceed based on the printer driver settings at the time.
     - The default values of the page-feeding method is "automatically select"
       with paper size set and "Letter", therefore please prepare Letter paper
       for the test page.
     - Change the setting when using a different size of paper for the test
       page.

k. When the installation is completed, an icon of the added printer will appear
   in the "Printers" folder.



4. Printer driver setup method

- The printer driver settings can be done by going to the "Printers" folder and
  select the printer, "File" - "Properties".

- Refer read the chapter of software in the user's manual for further details.



5. Others

a. The emulation for this driver is in the "DPL24C+" mode.
   Make sure the setting of the printer installation corresponds to it.

b. Users are required to adjust devices for such as the paper insertion.
   Please make sure the paper settings, as well as the settings from the
   operation panel correspond to the printer.

c. Printing from Windows3.1 application software under the Windows95
   environments may give different results.

d. Some specified printer fonts from the application may not be used depending
   on the data format.

e. Based on the application, zoom-in/out printing may always result in
   10.5-size fonts.

f. Paper with a length of 2.5 inches - 14 inches isruled with a width of 10
   inches.
   When using paper with a width less than 10 inches, please make adjustments
   to the right margin of the application not to exceed the maximum possible
   range.

g. When using Continuous form with a tractor feeder on this printer, the
   possible folding length is 4 inches or more.
   When the folding length is the same as the page length, use paper with a
   folding length of more than 4 inches.

h. If printing is cancelled from the printer port during printing, restart the
   printer.
   Continuing printing without restarting the printer may result in problems
   such as garbled texts.

i. Continuous Form
   - Both the upper and lower margins for continuous form are set at 0mm in
     this printer driver.  It is recommended that the upper and lower margins
     for continuous form using Tractor feeder with this printer is more than
     25.4mm
   - The printing head and the ribbon may be damaged when printing on the
     perforation lines and sprocket holes.

j. Envelopes
   - Print only on the surface side.  Do not print on the flap side as the
     envelope may be jammed.
   - Do not print on envelopes with a window or double-layered envelopes.
   - Both the top and bottom margins are set at 25.4mm in this printer driver.
   - Printing outside the margin out of guarantee.
   - Refer to the following for paper-feeding directions to avoid a paper jam.
          +---------------------------------------------------------+
          |*                                                       *|
          | *                                                     * |
          |  *          insert paper in this direction           *  |
          |   *                                                 *   |
          |    * * * * * * * * * * * * * * * * * * * * * * * * *    |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |  * * * * * * * * * * * * * * * * * * * * * * * * * * *  |
          | *                                                     * |
          |*                                                       *|
          +---------------------------------------------------------+

k. Adjust the paper guide when printing on B4(JIS) and B5(JIS) paper.
   (The left printing margin is set at 13.4mm)

l. A message "Please insert paper" will appear for every single page when the
   user selects to use the "Manual feed".  Click "OK" and proceed the printing.
   NOTE: For some applications, the message "Please insert paper" may not
         appear in the dialogue box.  Simply click the "OK" button and printing
         will proceed.

m. On multiple User-Defined sizes...
   Set up the printer driver for every User-Defined size.  The driver can be
   used interchangeably by entering the sizes as the driver names.

n. When Printer Font is specified and print it, change Language setting
   to PAGE850 by DLMENU or Offline Setup.
   Otherwise, print result may not be correct.



- About the trademark
    Company names and product names mentioned above are registered trademarks
    or trademarks of each company.

[End]
