===============================================================================
                       Microsoft Windows98/Me English

                       FUJITSU DL7400 Printer Driver

                                Version 3.10

                    Copyright(C) 2006 FUJITSU ISOTEC LIMITED
===============================================================================

This printer driver works with the following operating systems:

     Microsoft(R) Windows(R) 98 English
      -> referred to as Windows98
     Microsoft(R) Windows(R) 98 Second Edition English
      -> referred to as Windows98
     Microsoft(R) Windows(R) Millennium Edition English
      -> referred to as WindowsMe

This printer driver is for the FUJITSU DL7400 printers.



Contents

1. Printer driver operating environment
2. Printer driver configuration
3. Printer driver setup
  3.1 Before setting up
  3.2 Setup from "New Hardware Found"
    3.2.1 for Windows98
    3.2.2 for WindowsMe
  3.3 Setup from "Add Printer"
4. Setup of USB device driver
  4.1 for Windows98
  4.2 for WindowsMe
5. Printer driver setup method
6. Others
- About the trademark

NOTE: This driver is for FUJITSU DL7400 printers.
      Do not use it on other printers.
      When printing using Windows98 or WindowsMe, change the printer settings
      back to the factory default.
      Otherwise printer may not function as expected.



1. Printer driver operating environment

- Hardware
  PC's with the English-version Windows98 or WindowsMe

- Target operating system
  Windows98 (English-version) or WindowsMe (English-version)

NOTE:  This product only operates on English-version Windows98 or WindowsMe.



2. Printer driver configuration

  FUJITSU DL7400 printer driver consists of the following files:

   DL7400.DRV    FUJITSU DL7400 printer driver
   MGLMON.DLL    FUJITSU DL7400 Language Monitor
   DL7400.INF    Setup information file
   README.TXT    This file



3. Printer driver setup

---------------------
3.1 Before setting up
---------------------
- Prepare the following for setup:
   1) Windows98 or WindowsMe operating system  (CD-ROM)
   2) Printer Driver Disk                      (this disk)

- Set up FUJITSU DL7400 from "New Hardware Found".
  If "New Hardware" is not found, set up from "Add Printer".

- If the FUJITSU DL7400 printer driver has already been set up, delete
  it and set up again.


-----------------------------------
3.2 Setup from "New Hardware Found"
-----------------------------------
+++++++++++++++++++
3.2.1 For Windows98
+++++++++++++++++++
a. Connect the printer to the PC and turn on the PC.

b. Turn on the PC, and start Windows98.
   Restart Windows98 if it is already started.

c. When "Add New Hardware Wizard" appears, click "next".

d. Select "Search for the best driver for your device. (recommended)", and
   click "next".

e. Insert the printer driver setup disk into the CD drive.

f. Check "Specify a location", and enter "D:\Drivers\DL7400\English\Win98Me"
   (if D: is the CD drive), and click "next".

g. When the message "Windows driver file search for the device:" appears, click
   "next". 
   NOTE: When the dialogue "insert disk" appears, click "OK", enter
         "D:\Drivers\DL7400\English\Win98Me"(if the D: is the CD drive)
         into the "file copy source", and click OK.

h. Follow the instructions on the screen and continue with the setup.

i. When the message "the required software is installed into the "new hardware
   device." appears, click "finish".

  Printer driver setup is now complete.



+++++++++++++++++++
3.2.2 For WindowsMe
+++++++++++++++++++
a. Connect the printer to the PC, turn on the printer.

b. Turn on the PC and start WindowsMe.  Restart WindowsMe if already been
   started.

c. When "Add New Hardware Wizard" appears, click "next".

d. Insert the printer driver setup disk into the CD drive.

e. Select "auto driver-search (recommended)" and click on "next".
   Note: If "device software cannot be found" appears, click on "previous",
         and read directions from (5').

f. For details on location, select the driver from the "Win98Me" directory,
   and click "OK".

g. The "add printer wizard" will appear on the screen.

h. Follow the instructions and proceed.
   Note: If there is a conflict (if "there is a newer file than the one
         to be copied, and users are advised to use the already existing
         file" appears), click "yes".

i. When "the necessary software has been installed to the new hardware device"
   appears, click on "finish".

Printer driver setup is now complete.


Note: Specifying driver location:

f'. Select "specifying driver location", and click on "next".

g'. Check "specifying search location", enter "D:Drivers\DL7400\English\
    \Win98Me" (if D: is the CD drive), and click on "next".

h'. For details on location, select the drive from the "Win98Me" directory,
    and click "OK".

i'. When "driver file search: FUJITSU DL7400" appears, click "next".

j'. Follow the instructions and proceed.
    Note: If there is a conflict (if "there is a newer file than the one
          to be copied, and users are advised to use the already existing
          file" appears), click "yes".

k'. When "the necessary software has been installed to the new hardware
    device" appears, click "finish".



-----------------------------
3.3 Setup from "Aadd Printer"
-----------------------------
Here, both WindowsMe and Windows98 will be referred to as "Windows98":

a. Click on "My Computer" -> "Printers" -> "Add Printer".

b. The "Add Printer Wizard" will appear.  Follow the instructions on the screen
   and proceed.

c. When the printer list from the manufacturer appears click on "Have Disk".

d. Insert the printer setup disk into the CD drive, enter "D:\Drivers\DL7400
   \English\Win98Me" (if D: is the CD drive) as the "Copy manufacture's files
   from:", and click "OK".

e. The model names will be listed in the "Printers" list box.  Select the model
   and click  "next".
   NOTE: When the message "A driver is already installed for this printer.
         Would you like to keep the existing driver or use the new driver one?
         Your programs may print differently if you use the new driver",
         appears, select "Replace existing driver".

f. Select the "Available ports".

g. Confirm the printer name, and set it as the default printer, and click on
   "next".

h. Perform a printout test if desired, and select "Finish".
   NOTE: The user may be required to insert the Windows98 system CD-ROM.  Click
         "OK" after inserting the CD-ROM.  Enter "D:\WIN98" for the "Copy files
         from:" or click  "Browse" and select "D:\WIN98".

i. As in [h.], when "Print Test Page" is selected, a dialogue box will appear
   when printing is completed.  Click the "OK" or "No" button.
   Note with Test Page:
     - Printing will proceed based on the printer driver settings at the time.
     - The default values of the page-feeding method is "Manual Paper Feed"
       with paper size set and "Letter", therefore please prepare Letter paper
       for the test page.
     - Change the setting when using a different size of paper for the test
       page.

j. When the installation is completed, an icon of the added printer will appear
   in the "Printers" folder.

Printer driver setup is now complete.



4. Setup of USB device driver

Setup this USB device driver in the following process.
If setup is not done in the following process, it may not be able to
operate.

+++++++++++++++++
4.1 For Windows98
+++++++++++++++++
a. Turn the PC power on and start Windows 98.

b. Connect the PC with the DL7400 printer by USB cable.
   NOTE: Confirm that the DL7400 printer power is off when connecting the PC
         with the DL7400 printer by USB cable.
         If the PC and the DL7400 printer are not firmly connected by USB
         cable, the DL7400 printer cannot be detected.

c. Turn on the DL7400 printer power.

d. When "Add wizard to new hardware" appears, click "next".

e. Select the "Detect the most suitable driver for the device used
   (recommended)", and click "next".

f. Set the "FUJITSU DL7400 Printer Driver Disk" in the CD driver.

g. Check the "Designated detection area", input (D:\Drivers\DL7400\English
   \Win98Me)(if D: is the CD drive), then click "next".

h. Click "next" if the following messages appear:
     Detect the driver file for the following device use:
          USB Printing Support
     Installation of the most suitable driver for this device has been
     prepared.
   NOTE: If the "disk insertion" dialog box appears, then click "OK".
         Then input (D:\Drivers\DL7400\English\Win98Me) to the "File copy
         source", (if D: is the CD drive), and then click "OK".

i. Continue the setup of screen directions.

j. If "Necessary software for new hardware device has been installed"
   appears, click "finish".

For setup method, read the "3. Printer driver setup"


++++++++++++++
4.2 Windows Me
++++++++++++++
a. Turn the PC power on and start Windows Me.   

b. Connect the PC with the DL7400 printer by USB cable.
   NOTE: Confirm that the DL7400 printer power is off when connecting the PC
         with the DL7400 printer by USB cable.
         If the PC and the DL7400 printer are not firmly connected by USB
         cable, the DL7400 printer cannot be detected.

c. Turn the DL7400 printer power on.

d. When "Add wizard to new hardware" appears, FUJITSU DL7400 Printer Driver
   Disk to the CD driver is set.

e. Select the "Detect the most suitable driver for the device used
   (recommended))", and click "next".

f. If "New hardware device installation is finished" appears, click "finish".

For setup method, read the "3. Printer driver setup"



5. Printer driver setup method

- The printer driver settings can be done by going to the "Printers" folder and
  select the printer, "File" - "Properties".

- Refer read the chapter of software in the user's manual for further details.



6. Others

a. The emulation for this driver is in the "DPL24C+" mode.
   Make sure the setting of the printer installation corresponds to it.

b. Users are required to adjust devices for such as the paper insertion.
   Please make sure the paper settings, as well as the settings from the
   operation panel correspond to the printer.

c. Printing from Windows3.1 application software under the Windows98 and 
   WindowsMe environments may give different results.

d. Some specified printer fonts from the application may not be used depending
   on the data format.

e. Based on the application, zoom-in/out printing may always result in
   10.5-size fonts.

f. Paper with a length of 1 inches - 14 inches isruled with a width of 15
   inches.
   When using paper with a width less than 15 inches, please make adjustments
   to the right margin of the application not to exceed the maximum possible
   range.
   The paper length can be set starting from 1inch (about 25.4 mm).
   However, when specifying any of the paper feed ports below, do not specify
   paper 2.76 inches (about 70.0 mm) or less in length.
   Otherwise, the paper will not be properly fed, leading to a paper jam.

  - manual feed
  - CSF #1
  - CSF #2

g. When using Continuous form with a tractor feeder on this printer, the
   possible folding length is 4 inches or more.
   When the folding length is the same as the page length, use paper with a
   folding length of more than 4 inches.

h. If printing is cancelled from the printer port during printing, restart the
   printer.
   Continuing printing without restarting the printer may result in problems
   such as garbled texts.

i. Continuous Form
   - Both the upper and lower margins for continuous form are set at 0mm in
     this printer driver.  It is recommended that the upper and lower margins
     for continuous form using Tractor feeder with this printer is more than
     25.4mm
   - The printing head and the ribbon may be damaged when printing on the
     perforation lines and sprocket holes.

j. Envelopes
   - Print only on the surface side.  Do not print on the flap side as the
     envelope may be jammed.
   - Do not print on envelopes with a window or double-layered envelopes.
   - Printing outside the margin out of guarantee.
   - Refer to the following for paper-feeding directions to avoid a paper jam.
          +---------------------------------------------------------+
          |*                                                       *|
          | *                                                     * |
          |  *          insert paper in this direction           *  |
          |   *                                                 *   |
          |    * * * * * * * * * * * * * * * * * * * * * * * * *    |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |  * * * * * * * * * * * * * * * * * * * * * * * * * * *  |
          | *                                                     * |
          |*                                                       *|
          +---------------------------------------------------------+

k. Adjust the paper guide when printing on A3 Rotated paper.
   (The left printing margin is set at 38mm)

l. A message "Please insert paper" will appear for every single page when the
   user selects to use the "Manual feed".  Click "OK" and proceed the printing.
   NOTE: For some applications, the message "Please insert paper" may not
         appear in the dialogue box.  Simply click the "OK" button and printing
         will proceed.

m. On multiple User-Defined sizes...
   Set up the printer driver for every User-Defined size.  The driver can be
   used interchangeably by entering the sizes as the driver names.

n. When Printer Font is specified and print it, change Language setting
   to WCP1252 by DLMENU or Offline Setup.
   Otherwise, print result may not be correct.

o. Regarding the DL7400 Printer
   Ejecting cut sheet paper to the cut sheet table in front sometimes leads to
   wait for removal of a cut sheet (blinking lamp for ejection in front).
   In such cases, remove the paper from the cut sheet table, load the next
   paper, and then press the online switch.

   **The error message displayed when status of wait for removal of a cut
   sheet (blinking lamp for ejection in front) occurs during printing
   indicates a time out error, not a paper out error.

- About the trademark
    Company names and product names mentioned above are registered trademarks
    or trademarks of each company.

[End]
