===============================================================================

                       Microsoft WindowsNT4.0 English

                       FUJITSU DL7400 Printer Driver

                                 Version 3.10

                   Copyright(C) 2006 FUJITSU ISOTEC LIMITED

===============================================================================

This printer driver works on the following operating systems:

  Microsoft(R) Windows NT(R) 4.0 English (referred to as WindowsNT4.0)

This printer driver is for FUJITSU DL7400 printers.



Contents

1. Printer driver operating environment
2. Printer driver configuration
3. Printer driver setup
  3.1 Before setting up
  3.2 Setup method
4. Printer driver setup method
5. Others
- About the trademark

Note: This driver is for FUJITSU DL7400 printers.
      Do not use with other printers.
      When printing using WindowsNT4.0, change the printer settings back to the
      factory default.
      Otherwise printer may not function as expected.



1. Printer driver operating environment

- Hardware
  PC's with the English-version WindowsNT4.0

- Operating system
  WindowsNT4.0 (English-version)

NOTE: This product only operates on English-version WindowsNT4.0.



2. Printer driver configuration

   FUJITSU DL7400 printer driver consists of the following files:

   DL7400.DLL     FUJITSU DL7400 printer driver resource DLL file
   MGLMONN.DLL    FUJITSU DL7400 Language Monitor
   DL7400.INF     Setup information file
   README.TXT     This file



3. Printer driver setup
---------------------
3.1 Before setting up
---------------------
- Prepare the following for setup:
   1) English-version WindowsNT Workstation4.0 or WindowsNT Server4.0
      operating system (CD-ROM)
   2) Printer Driver Disk (this disk)

- When setting up, log on with an Administrator account.

- The printer driver for FUJITSU DL7400 cannot be installed as an
  alternative driver.

- Do not select "Sharing" when installing the printer driver.

- If the FUJITSU DL7400 printer driver has already been set up, delete
  it and set up again.



----------------
3.2 Setup method
----------------
Start setting up the printer driver by activating the "Add Printer Wizard".
The following is the FUJITSU DL7400 setup procedure after WindowsNT4.0
is started up.


a. Go to "My Computer" -> "Printers".

b. Double-click "Add Printer".

c. When "Add Printer Wizard" appears, select "My Computer", and click "next".

d. Specify an available port ("Add Port" and "Configure Port" if necessary),
   and click "next".

e. Click "Have Disk...", and a dialogue box "Install From Disk" will appear.

f. Insert the FUJITSU DL7400 driver disk, and enter "D:\Drivers\DL7400
   \English\Winnt40" as  the "Copy manufacture's files from:", and click OK.
   Note: The CD drive above is assumed to be D:, make changes if necessary.

g. The model names will be listed in the "printers" list box.  Select the model
   and click on "next".
   NOTE: When the message "A driver is already installed for this printer.
         Would you like to keep the existing driver or use the new driver one?
         Your programs may print differently if you use the new driver",
         appears, select "Replace existing driver".

h. Enter the printer model name, and specify whether the printer will be used
   as the default printer, and select "next".

i. Select "not shared" for the specified printer, and click "next".

j. Perform a printout test if desired, and select "next".
   NOTE: The user may be required to insert the WindowsNT4.0 system CD-ROM.
         Click "OK" after inserting the CD-ROM.  Enter "D:\I386" (if D: is
         the CD-ROM drive)for the "Copy files from:" or click  "Browse" and
         select "D:\I386".

k. After installation, return to the "Printers" dialogue box.
   Make sure the printer has been added in the "Printers" dialogue box.

l. As in [j.], when "Print Test Page" is selected, a dialogue box will appear
   when printing is completed.  Click the "Yes" or "No" button.
   Note with Test Page:
     - Printing will proceed based on the printer driver settings at the time.
     - The default values of the page-feeding method is "automatically select"
       with paper size set and "Letter", therefore please prepare Letter paper
       for the test page.
     - Change the setting when using a different size of paper for the test
       page.

m. Go to "File" from the menu bar and select "Close" to close the dialogue box.

Printer driver setup is now completed.



4. Printer driver setup method

- The printer driver settings can be adjusted by going to the "Printers" folder
  and selecting the printer then going to "File" - "Document Defaults" or by
  going to "Properties" - "Device settings".

- Refer read the chapter of software in the user's manual for further details.



5. Others

a. The emulation for this driver is in the "DPL24C+" mode.
   Make sure the setting of the printer installation corresponds to it.

b. Users are required to adjust devices for such as the paper insertion.
   Please make sure the paper settings, as well as the settings from the
   operation panel correspond to the printer.

c. Printing from Windows95 application software under the WindowsNT4.0
   environments may give different results.

d. The contents of "Properties" of the printer driver and "Printing
   Preferences" of the printer may overlap.  Please make necessary adjustments
   to avoid any possible malfunction.

e. Some specified printer fonts from the application may not be used depending
   on the data format.

f. Paper size from the "Server Properties" can be set to a maximum width of
   15 inches.  Adjust the right and left margins not the exceed an 13.6 inch
   paper width as the data may not be properly printed.
   The paper length can be set starting from 1inch (about 25.4 mm).
   However, when specifying any of the paper feed ports below, do not specify
   paper 2.76 inches (about 70.0 mm) or less in length.
   Otherwise, the paper will not be properly fed, leading to a paper jam.

   - manual feed
   - CSF #1
   - CSF #2

g. Based on the application, zoom-in/out printing may always result in
   10.5-size fonts.

h. Paper with a length of 1 inches - 14 inches isruled with a width of 15
   inches.
   When using paper with a width less than 15 inches, please make adjustments
   to the right margin of the application not to exceed the maximum possible
   range.

i. When using Continuous form with a tractor feeder on this printer, the
   possible folding length is 4 inches or more.
   When the folding length is the same as the page length, use paper with a
   folding length of more than 4 inches.

j. If printing is cancelled from the printer port during printing, restart the
   printer.
   Continuing printing without restarting the printer may result in problems
   such as garbled texts.

k. Continuous Form
   - Both the upper and lower margins for continuous form are set at 0mm in
     this printer driver.  It is recommended that the upper and lower margins
     for continuous form using Tractor feeder with this printer is more than
     25.4mm
   - The printing head and the ribbon may be damaged when printing on the
     perforation lines and sprocket holes.

l. Envelopes
   - Print only on the surface side.  Do not print on the flap side as the
     envelope may be jammed.
   - Do not print on envelopes with a window or double-layered envelopes.
   - Printing outside the margin out of guarantee.
   - Refer to the following for paper-feeding directions to avoid a paper jam.
          +---------------------------------------------------------+
          |*                                                       *|
          | *                                                     * |
          |  *          insert paper in this direction           *  |
          |   *                                                 *   |
          |    * * * * * * * * * * * * * * * * * * * * * * * * *    |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |  * * * * * * * * * * * * * * * * * * * * * * * * * * *  |
          | *                                                     * |
          |*                                                       *|
          +---------------------------------------------------------+

m. Adjust the paper guide when printing on A3 Rotated paper.
   (The left printing margin is set at 38mm)

n. When Printer Font is specified and print it, change Language setting
   to WCP1252 by DLMENU or Offline Setup.
   Otherwise, print result may not be correct.

o. Regarding the DL7400 Printer
   Ejecting cut sheet paper to the cut sheet table in front sometimes leads to
   wait for removal of a cut sheet (blinking lamp for ejection in front).
   In such cases, remove the paper from the cut sheet table, load the next
   paper, and then press the online switch.

   **The error message displayed when status of wait for removal of a cut
   sheet (blinking lamp for ejection in front) occurs during printing
    indicates a time out error, not a paper out error.

p. Changing the paper feed port or paper size with the page setting or
   document setting in the application
   The margin size outside the print enabled area can be set even when the
   printer driver specified value is not correctly reflected.
   To prevent this, first set the paper feed port and paper size you intend to
   use with printer properties in the printer folder.  Then change the paper
   feed port and paper size in the application, or avoid setting the margin
   size outside the print enabled area.  For information on the print enabled
   area (minimal margin size) per individual paper feed ports and paper sizes,
   refer to the Users Manual.

- About the trademark
    Company names and product names mentioned above are registered trademarks
    or trademarks of each company.

[End]
