===============================================================================
                             Microsoft Windows2003

                         FUJITSU DL7600 Printer Driver

                    Copyright(C) 2010 FUJITSU ISOTEC LIMITED
===============================================================================

This printer driver works on the following operating systems:

     Microsoft(R) Windows Server(R) 2003 Standard Edition
     Microsoft(R) Windows Server(R) 2003 Standard x64 Edition
     Microsoft(R) Windows Server(R) 2003 Enterprise Edition
     Microsoft(R) Windows Server(R) 2003 Enterprise x64 Edition
      -> referred to as Windows2003

This printer driver is for FUJITSU DL7600 printers.


Content

1. Printer driver operating environment
2. Printer driver configuration
3. Printer driver setup
  3.1 Before setting up
  3.2 Setup method using Add Printer Wizard (without using Plug & Play)
  3.3 Setup method using Add Printer Wizard (using Plug & Play)
  3.4 Using Plug & Play
4. Uninstallring the printer driver
5. Printer driver setup method
6. Others
- About the trademark

Note: This driver is for FUJITSU DL7600 printers.
      Do not use with other printers.
      When printing using Windows2003, change the printer settings back to the
      factory default.
      Otherwise printer may not function as expected.



1. Printer driver operating environment

- Hardware
  PC's with the English-version Windows2003

- Operating system
  Windows2003 (English-version)

NOTE:  This product only operates on English-version Windows2003.



2. Printer driver configuration

  FUJITSU DL7600 printer driver consists of the following files:

   DL7600.GPD     FUJITSU DL7600 printer driver GPD file
   DL7600.DLL     FUJITSU DL7600 printer driver resource DLL file
   HGLMONN.DLL    FUJITSU DL7600 Language Monitor
   DL7600.INF     Setup information file
   README.TXT     This file



3. Printer driver setup

---------------------
3.1 Before setting up
---------------------
- Prepare the following for setup:
   1) English-version Windows2003 operating system
   2) Printer Driver Disk (this disk)

- When setting up, log on with an Administrator account.

- Before setting up, go to System Properties, select <ignore> or <warn> for the
  "Driver Signing" at the driver signing options.

- If the FUJITSU DL7600 printer driver has already been set up, delete
  it and set up again.

- This guide includes procedures on installing printer drivers on locally
  connected PC's.
  For installation methods on network connection and shared printers, refer to
  the Windows2003 user's manual or "help".


---------------------------------------------------------------------
3.2 Setup method using add-printer wizard (without using Plug & Play)
---------------------------------------------------------------------
Start Add Printer Wizard.
The following is the FUJITSU DL7600 setup procedure after Windows2003
is started up.

a. Go to "Start" -> "Printers and Faxes".

b. Select "Add a printer".

c. When "Add Printer Wizard" appears, select "next".

d. When "Local or Network Printer" in "Add Printer Wizard" appears, select
   "Local printer attached to this computer", un-check "Automatically detect
   and install my Plug & Play printer", and select "next".

e. Specify the connecting port for the printer, and select "next".

f. Click the "Have Disk..." button.

g. Insert this disk into the CD drive (if D: is the CD drive), change the path
   from "A:\" to "D:\Drivers\DL7600\English\Win2003", and press "OK".
   NOTE: The CD drive above is assumed to be D:, make changes if necessary.

h. The model names will be shown in the list box.
   Choose the model used and press "next".
   NOTE: When the message "Do you want to keep the existing driver or use the
         new one?" Appears, select "Replace existing driver".

i. Enter the printer model name , and specify whether the printer will be used
   as the default printer, and select "next".

j. Specify if the printer will be shared, and select "next".
   Enter the shared name if it will be shared.
   Go to [l.] if it is not shared.

k. Select whether the printer location and comment provider are desired, and
   click "next".

l. After installation is completed, print test page if desired, and select
   "next".

m. To end the wizard, click the "Finish" button.

n. When the screen "Hardware Installation" appears, select "Continue Anyway".
   NOTE: As in 3.1, this is the case when the "Driver Signing" is set to
   "Warn".

o. The files are copied and the installation for the driver is now completed.
   In [l.], when "Print Test Page" is selected, a dialogue box to inform the
   printing complete will appear when printing is completed.  click the "Yes"
   or "Troubleshoot..." button.
   Note  with Test Page:
     - Printing will proceed based on the printer driver settings at the time.
     - The default settings for the printer driver are "Automatically Select"
       for the paper feed method, and "11 inch Stockform(W:15in)" for the
       paper size, so insert 11 x 15 inch Stockform paper before printing
       the test page.
     - Change the setting when using a different size of paper for the test
       page.

Printer driver setup is now complete.


-------------------------------------------------------------
3.3 Setup method using add-printer wizard (using Plug & Play)
-------------------------------------------------------------
Start Add Printer Wizard.
The following is the setup procedure after Windows2003 is started up.
Note: Turn on the printer.

a. Go to "Start" -> "Printers and Faxes".

b. Select "Add Printer".

c. When "Add Printer Wizard" appears, select "next".

d. When "Local or Network Printer" in "Add Printer Wizard" appears, select
   "Local printer attached to this computer", check "Automatically detect and
   install my Plug & Play printer", and select "next".

e. "Found New Hardware Wizard" will appear on the screen.  Insert the printer
   driver disk, select "Install from a list or specific location (Advanced)",
   and select "next".

f. When "Please choose your search and installation options" appears, select
   "Search for the best driver in these locations.", un-check "Search removable
   media (floppy,CD-ROM...)", and only check "Include this location in the
   search".  Enter "D:\Drivers\DL7600\English\Win2003" and select "next".
   NOTE: The CD drive above is assumed to be D:, make changes if necessary.

g. File copy start.

m. When the screen "Hardware Installation" appears, select "Continue Anyway".
   NOTE: As in 3.1, this is the case when the "Driver Signing" is set to
         "Warn".

i. When "Completing the Found New Hardware Wizard" appears, make sure the
   message "The wizard has installing the software for : FUJITSU DL7600"
   appears, and select "Finish".

j. When "New Printer Detection" appears on the screen, Make sure the message
   "Do you want to a test page?" appears.
   Select "Yes" or "No", and select "next".

k. When "Completing the Add Printer Wizard" appears on the screen, make sure
   the message "You have successfully completed the Add Printer Wizard. You
   specified the following printer settings" appears. Select "Finish".

l. The files are copied and the installation for the driver is now completed.
   In [j.], when "Print Test Page" is selected, a dialogue box to inform the
   printing complete will appear when printing is completed.  click the "Yes"
   or "Troubleshoot..." button.
   Note  with Test Page:
     - Printing will proceed based on the printer driver settings at the time.
     - The default settings for the printer driver are "Automatically Select"
       for the paper feed method, and "11 inch Stockform(W:15in)" for the
       paper size, so insert 11 x 15 inch Stockform paper before printing
       the test page.
     - Change the setting when using a different size of paper for the test
       page.

m. When installation is complete, an icon of the added printer will appear in
   the "Printers and Faxes" folder.

Printer driver setup is now complete.


---------------------
3.4 Using Plug & Play
---------------------
NOTE: Turn off both the PC and the printer.

a. Make sure the printer is connected to the PC, and turn on the printer.

b. Make sure the printer is on-line, turn on the PC, and start Windows2003.

c. "Welcome to the Found New Hardware Wizard" will appear on the screen.
   Insert the printer driver disk, select "Install from a list or specific
   location (Advanced)", and select "next".

d. When "Please choose your search and installation options" appears, select
   "Search for the best driver in these locations.", un-check "Search removable
   media (floppy,CD-ROM...)", and only check "Include this location in the
   search".  Enter "D:\Drivers\DL7600\English\Win2003" and select "next".
   NOTE: The CD drive above is assumed to be D:, make changes if necessary.

e. When the screen "Hardware Installation" appears, select "Continue Anyway".
   NOTE: As in 3.1, this is the case when the "Driver Signing" is set to
         "Warn".

f. File copy start.

g. When "Completing the Found New Hardware Wizard" appears, make sure the
   message "The wizard has installing the software for : FUJITSU DL7600"
   appears, and select "Finish".

Printer driver setup is now complete.



4. Uninstalling the printer driver

Printer driver uninstallation is as follows.

a. Go to "Start" -> "Printers and Faxes".

b. Select "FUJITSU DL7600" from the "Printers and Faxes" folder, and select
   "Delete" from the "File" menu.

c. When "Are you sure want to delete the printer 'FUJITSU DL7600'?" appears on
   the screen, select "yes".
   NOTE: If the printer driver is not installed, "Warning: The default printer
         has beeb deleted.  There are printers set up on your computer." will
         appear.  Press the "OK" button.
         If there is no default printer, the message "Warning: The default
         printer has been deleted. The new printer is 'XXXXXX XXXXXXX'
         ('XXXXX XXXXXX' being the newly installed printer) will appear on
         the screen.  Press the "OK" button.

d. Select "Server Properties" from the "File" menu, click on the "Drivers" tab.

e. Select "FUJITSU DL7600" from the "Installed printer drivers:" list, and
   select "Remove".

f. When "Deleting this printer driver will remove it from the system.
   Are yousure you want to delete FUJITSU DL7600?" appears on the screen,
   select "Yes".

g. After the drive is deleted, click on "Close" and terminate the "Print Server
   Properties" dialogue.

h. Turn off the printer and restart the computer.

Printer driver is now removed.



5. Printer driver setup method

- Document properties such as paper size and others can be set in the "printer
  properties" menu in the application software.

- Depending on the application software used, the paper size settings of the
  application software may be the default rather than that of the "page
  setting" tab.

- The following is the method for each paper feeding (to set such as paper size
  assignment):
  Select "Start" -> "Printers and Faxes" -> "FUJITSU DL7600" and click on the
  right button of the mouse, select "properties",
  specify the "Form to Tray assignment" from the "Device Settings" tab.

  NOTE:
  - This method is valid only when the Paper Source setting of the printer
    driver is set at the "Automatically Select".
  - Please make sure the actual paper size matches the selected paper size.
    Use the "Manual Paper Feed" the actual paper size differs from the selected
    paper size.

- Refer read the chapter of software in the user's manual for further details.



6. Others

a. The emulation for this driver is in the "DPL24C+" mode.
   Make sure the setting of the printer installation corresponds to it.

b. Users are required to adjust devices for such as the paper insertion.
   Please make sure the paper settings, as well as the settings from the
   operation panel correspond to the printer.

c. Printing from Windows95 application software under the Windows2003
   environments may give different results.

d. The contents of "Properties" of the printer driver and "Printing
   Preferences" of the printer may overlap.  Please make necessary adjustments
   to avoid any possible malfunction.

e. Some specified printer fonts from the application may not be used depending
   on the data format.

f. Paper size from the "Server Properties" can be set to a maximum width of
   15 inches.  Adjust the right and left margins not the exceed an 13.6 inch
   paper width as the data may not be properly printed.

   The paper length can be set starting from 1inch (about 25.4 mm).
   However, when specifying any of the paper feed ports below, do not specify
   paper 2.76 inches (about 70.0 mm) or less in length.
   Otherwise, the paper will not be properly fed, leading to a paper jam.
   - manual feed
   - CSF #1
   - CSF #2

g. When printing with a "Page per Sheet" specification from the "layout" tab in
   the print menu, frame lines may not be printed with some applications.

h. Based on the application, zoom-in/out printing may always result in
   10.5-size fonts.

i. Paper with a length of 3 inches - 14 inches isruled with a width of 15
   inches.
   When using paper with a width less than 15 inches, please make adjustments
   to the right margin of the application not to exceed the maximum possible
   range.

j. When using Continuous form with a tractor feeder on this printer, the
   possible folding length is 4 inches or more.
   When the folding length is the same as the page length, use paper with a
   folding length of more than 4 inches.

k. If printing is cancelled from the printer port during printing, restart the
   printer.
   Continuing printing without restarting the printer may result in problems
   such as garbled texts.

l. Continuous Form
   - Both the upper and lower margins for continuous form are set at 0mm in
     this printer driver.  It is recommended that the upper and lower margins
     for continuous form using Tractor feeder with this printer is more than
     25.4mm
   - The printing head and the ribbon may be damaged when printing on the
     perforation lines and sprocket holes.

m. Envelopes
   - Print only on the surface side.  Do not print on the flap side as the
     envelope may be jammed.
   - Do not print on envelopes with a window or double-layered envelopes.
   - Printing outside the margin out of guarantee.
   - Refer to the following for paper-feeding directions to avoid a paper jam.
          +---------------------------------------------------------+
          |*                                                       *|
          | *                                                     * |
          |  *          insert paper in this direction           *  |
          |   *                                                 *   |
          |    * * * * * * * * * * * * * * * * * * * * * * * * *    |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |  * * * * * * * * * * * * * * * * * * * * * * * * * * *  |
          | *                                                     * |
          |*                                                       *|
          +---------------------------------------------------------+

n. Adjust the paper guide when printing on A3 Rotated paper.
   (The left printing margin is set at 38mm)

o. The DL7600 printer driver to every connecting port will be set if the
   connecting USB port is changed.  (e.g. FUJITSU DL7600 (copy 2) etc.)
   Since every setting of the printer driver is the initial value, so
   change the setting according to the using state.

p. When Printer Font is specified and print it, change Language setting
   to WCP1252 by DLMENU or Offline Setup.
   Otherwise, print result may not be correct.

q. Regarding the DL7600 Printer
   Ejecting cut sheet paper to the cut sheet table in front sometimes leads to
   wait for removal of a cut sheet (blinking lamp for ejection in front).
   In such cases, remove the paper from the cut sheet table, load the next
   paper, and then press the online switch.

   **The error message displayed when status of wait for removal of a cut
   sheet (blinking lamp for ejection in front) occurs during printing 
   indicates a time out error, not a paper out error.

r. Changing the paper feed port or paper size with the page setting or
   document setting in the application.
   The margin size outside the print enabled area can be set even when the
   printer driver specified value is not correctly reflected.
   To prevent this, first set the paper feed port and paper size you intend to
   use with printer properties in the printer folder.  Then change the paper
   feed port and paper size in the application, or avoid setting the margin
   size outside the print enabled area.  For information on the print enabled
   area (minimal margin size) per individual paper feed ports and paper sizes,
   refer to the Users Manual.

- About the trademark
    Company names and product names mentioned above are registered trademarks
    or trademarks of each company.

[End]
