===============================================================================
                             Microsoft Windows2000
                             Microsoft WindowsXP

                         FUJITSU DL7400 Printer Driver

                    Copyright(C) 2010 FUJITSU ISOTEC LIMITED
===============================================================================

This printer driver works on the following operating systems:

  Microsoft(R) Windows(R) 2000 English
  -> referred to as Windows2000

  Microsoft(R) Windows(R) XP Professional
  Microsoft(R) Windows(R) XP Professional x64 Edition
  Microsoft(R) Windows(R) XP Home Edition
  -> referred to as WindowsXP

This printer driver is for FUJITSU DL7400 printers.


Content

1. Printer driver operating environment
2. Printer driver configuration
3. Printer driver setup
  3.1 Before setting up
  3.2 for Windows2000
    3.2.1 Setup method using Add Printer Wizard (without using Plug & Play)
    3.2.2 Setup method using Add Printer Wizard (using Plug & Play)
    3.2.3 Using Plug & Play
  3.3 for WindowsXP
    3.3.1 Setup method using Add Printer Wizard (without using Plug & Play)
      3.3.1.1 for WindowsXP Professional 
      3.3.1.2 for WindowsXP Home Edition
    3.3.2 Setup method using add-printer wizard (using Plug & Play)
      3.3.2.1 for WindowsXP Professional
      3.3.2.2 for WindowsXP Home Edition
    3.3.3 Using Plug & Play
4. Uninstallring the printer driver
  4.1 Windows2000
  4.2 WindowsXP Professional
  4.3 WindowsXP Home Edition
5. Printer driver setup method
6. Others
- About the trademark

Note: This driver is for FUJITSU DL7400 printers.
      Do not use with other printers.
      When printing using Windows2000 or WindowsXP, change the printer settings
      back to the factory default.
      Otherwise printer may not function as expected.



1. Printer driver operating environment

- Hardware
  PC's with the English-version Windows2000 or WindowsXP

- Operating system
  Windows2000 (English-version) or WindowsXP (English-version)

NOTE: This product only operates on English-version Windows2000 and WindowsXP.



2. Printer driver configuration

  FUJITSU DL7400 printer driver consists of the following files:

   DL7400.GPD     FUJITSU DL7400 printer driver GPD file
   DL7400.DLL     FUJITSU DL7400 printer driver resource DLL file
   MGLMONN.DLL    FUJITSU DL7400 Language Monitor
   DL7400.INF     Setup information file
   README.TXT     This file



3. Printer driver setup

---------------------
3.1 Before setting up
---------------------
- Prepare the following for setup:
   1) English-version Windows2000 or WindowsXP operating system
   2) Printer Driver Disk (this disk)

- When setting up, log on with an Administrator account.

- Before setting up, go to System Properties, select <ignore> or <warn> for the
  "file signature verification" at the driver signature options.

- If the FUJITSU DL7400 printer driver has already been set up, delete
  it and set up again.


--------------------
3.2 for Windows 2000
--------------------
++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
3.2.1 Setup method using Add Printer Wizard  (without using Plug & Play)
++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
Start Add Printer Wizard.
The following is the FUJITSU DL7400 setup procedure after Windows2000
is started up.

a. Go to "Start" -> "Settings" -> "Printers".

b. Double-click the "Add Printer" icon in the "Printers" folder.

c. When "Add Printer Wizard" appears, select "next".

d. When "local or network printer" from "Add Printer Wizard" appears, select
   "local printer", un-check "automatically detect and install my Plug and
   Play printer", and select "next".

e. Select the connecting port for the printer from "use the following port",
   and select "next".

f. When the printer list of each manufacturer appears click on "Have Disk...",
   insert the printer driver disk, enter the disk drive name "D:\Drivers
   \DL7400\English\Win2kxp" as the "Copy manufacture's files from:",
   and select "OK".
   Note: The CD drive above is assumed to be D:, make changes if necessary.

g. The model names will be listed in the "printers" list box.  Select the model
   and click on "next".
   Note: When the message "Use Existing Driver" appears, select "Replace
         existing driver".

h. Enter the printer model name, and specify whether the printer will be used
   as the default printer, and select "next".
   Note: The printer will be set automatically as the default printer if no
         other printers are installed.

i. Specify if the printer will be shared, and select "next".

j. Perform a printout test if desired, and select "next".

k. When the message "Completing the Add Printer Wizard", make sure the selected
   contents are correct, and select "finish".

l. When the message "digital signature not found" appears, select "yes".
   Note: As in 3.1, this is the case when the "file signature verification" is
         set to "warn".

m. The files are copied and the driver installation for the driver is now
   completed.

n. As in [j.], when "Print Test Page" is selected, a dialogue box will appear
   when printing is completed.  Click the "OK" or "troubleshoot" button.
   Note with Test Page:
     - Printing will proceed based on the printer driver settings at the time.
     - The default values of the page-feeding method is "automatically select"
       with paper size set and "Letter", therefore please prepare Letter paper
       for the test page.
     - Change the setting when using a different size of paper for the test
       page.

o. When installation is complete, an icon of the added printer will appear in
   the "Printers" folder.

Printer driver setup is now complete.


+++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
3.2.2 Setup method using add-printer wizard (using Plug & Play)
+++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
Start the Add Printer Wizard.
The following is the setup procedure after Windows 2000 is started up.
Note: Turn on the printer.

a. Go to "Start" -> "Settings" -> "Printers".

b. Double-click the "Add Printer" icon in the "Printers" folder.

c. When "Add Printer Wizard" appears, select "next".

d. When "local or network printer" from "add-printer wizard" appears, select
   "local printer", check "automatically detect and install my Plug and Paly
   printer", and select "next".

e. "New printer detection" will be activated, if successfully found, the
   dialogue "found new hardware" will appear.

f. When the message "Welcome to the Found New Hardware Wizard" from the "Found
   new hardware wizard" appears, select "next".

g. When the message "Install Hardware Device Drivers" from the "Found New
   Hardware wizard" appears, make sure "search for a suitable driver for my
   device (recommended)" is selected, and select "next".

h. When the screen "Locate Driver Files" appears, insert the Printer Driver
   Disk, and un-check "floppy disk drives" and "CD-ROM drives".  Make sure
   only "specify a location" is checked, and select "next".

i. Enter the disk drive name "D:\Drivers\DL7400\English\Win2kxp" in the
   "Copy manufacture's files from:", and select "OK".
   NOTE: The CD drive above is assumed to be D:, make changes if necessary.

j. When "Driver Files Search Results" appears, make sure the message "Windows
   found a driver for this device. To install the driver Windows found, click
   next." appears, and select "next".

k. When the message "digital signature not found" appears, select "yes".
   NOTE: As in 3.1, this is the case when the "file signature verification" is
   set to "warn".

l. File copy starts.

m. When the "Completiong the Found New Hardware Wizard" appears, make sure the
   message "Windows has finished installing the software for this device"
   appears, and select "finish".

n. When "New Printer Detection" appears on the screen, Make sure the message
   "Do you want to print a test page?" appears.  Select "yes" or "no", and
   select "next".

o. When "Completing the Add Printer Wizard" appears on the screen, make sure
   the message "You have successfully completed the Add Printer Wizard"
   appears.  Select "finish".

p. As in [n.], when "Print Test Page" is selected, a dialogue box will appear
   when printing is completed.  Click the "OK" or "troubleshoot" button.
   Note with Test Page:
     - Printing will proceed based on the printer driver settings at the time.
     - The default values of the page-feeding method is "automatically select"
       with paper size set and "Letter", therefore please prepare Letter paper
       for the test page.
     - Change the setting when using a different size of paper for the test
       page.

q. When installation is complete, an icon of the added printer will appear in
   the "Printers" folder.

Printer driver setup is now completed.
If the installation cannot be executed, refer to "3.2.1 Setup method using
Add Printer Wizard (without using Plug & Play)".


+++++++++++++++++++++++
3.2.3 Using Plug & Play
+++++++++++++++++++++++
NOTE: Turn off both the PC and the printer.

a. Make sure the printer is connected to the PC, and turn on the printer.

b. Make sure the printer is on-line, turn on the PC, and start up Windows2000.

c. "Found New Hardware" starts.
   A dialogue "Installing..." will appear if it is found.

d. When the "Found New Hardware Wizard" appears, select "next".

e. When the message "Install Hardware Device Drivers" from the "Found New
   Hardware Wizard" appears, make sure "search for a suitable driver for my
   device (recommended)" is selected, and select "next".

f. When the screen "Locate Driver Files" appears, insert the Printer Driver
   Disk, and un-check "floppy disk drives" and "CD-ROM drives".  Make sure
   only "specify a location" is checked, and select "next".

g. Enter the disk drive name "D:\Drivers\DL7400\English\Win2kxp" to the
   "Copy manufacture's files from:", and select "OK".
   NOTE: The CD drive above is assumed to be D:, make changes if necessary.

h. When "Driver Files Search Results" appears, make sure the message "Windows
   found a driver for this device. To install the driver Windows found, click
   next." appears, and select "next".

i. When the message "digital signature not found" appears, select "yes".
   NOTE: As in 3.1, this is the case when the "file signature verification" is
   set to "warn".

j. File copy starts.

k. When the "Completiong the Found New Hardware Wizard" appears, make sure the
   message "Windows has finished installing the software for this device"
   appears, and select "finish".

Printer driver setup is now complete.


-----------------
3.3 for WindowsXP
-----------------
+++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
3.3.1 Setup method using add-printer wizard (without using Plug & Play)
+++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++

3.3.1.1 for WindowsXP Professional
==================================
Start Add Printer Wizard.
The following is the FUJITSU DL7400 setup procedure after WindowsXP is
started up.

a. Go to "Start" -> "Control Panel" -> "Printers and Other Hardware".

b. Select "Add Printer".

c. When "Add Printer Wizard" appears, select "next".

d. When "Local or Network Printer" in "Add Printer Wizard" appears, select
   "Local printer attached to this computer", un-check "Automatically detect
   and install my Plug & Play printer", and select "next".

e. Specify the connecting port for the printer, and select "next".

f. Click the "Have Disk..." button.

g. Insert this disk into the CD drive (if D: is the CD drive), change the path
   from "A:\" to "D:\Drivers\DL7400\English\Win2kxp", and press "OK".
   NOTE: The CD drive above is assumed to be D:, make changes if necessary.

h. The model names will be shown in the list box.
   Choose the model used and press "next".
   NOTE: When the message "Do you want to keep the existing driver or use the
         new one?" Appears, select "Replace existing driver".

i. Enter the printer model name , and specify whether the printer will be used
   as the default printer, and select "next".

j. Specify if the printer will be shared, and select "next".

k. After installation is completed, print test page if desired, and select
   "next".

l. To end the wizard, click the "Finish" button.

m. When the screen "Hardware Installation" appears, select "Continue Anyway".
   NOTE: As in 3.1, this is the case when the "Driver Signing" is set to
         "Warn".

n. The files are copied and the installation for the driver is now completed.
   In [k.], when "Print Test Page" is selected, a dialogue box to inform the
   printing complete will appear when printing is completed.  click the "Yes"
   or "Troubleshoot..." button.
   Note  with Test Page:
     - Printing will proceed based on the printer driver settings at the time.
     - The default values of the page-feeding method is "automatically select"
       with paper size set and "Letter", therefore please prepare Letter paper
       for the test page.
     - Change the setting when using a different size of paper for the test
       page.

Printer driver setup is now complete.

3.3.1.2 for WindowsXP Home Edition
==================================
Start Add-printer Wizard.
The following is the setup procedure after WindowsXP Home Edition is started.

a. Go to "Start" -> "Control Panel" -> "Printer and other hardware".

b. Select "Add Printer" from the "Printer and other hardware" screen.

c. When the "Add Printer Wizard" screen appears, select "next".

d. When "Local or Network Printer" in "Add Printer Wizard" appears, select
   "Local printer attached to this computer", un-check "Automatically detect
   and install my Plug & Play printer", and select "next".

e. For the rest of the procedure, please refer to procedure [e.] and thereafter
   in "3.3.1.1 for WindowsXP Professional".

f. After installation, an icon of the added printer will appear in the
   "Printers and Faxes" folder.

Printer driver setup is now complete.


+++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++
3.3.2 Setup method using add-printer wizard (using Plug & Play)
+++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++++

3.3.2.1 for WindowsXP Professional
==================================
Start Add Printer Wizard.
The following is the setup procedure after WindowsXP Professional is
started up.
Note: Turn on the printer.

a. Go to "Start" -> "Control Panel" -> "Printer and other hardware".

b. Select "Add Printer".

c. When "Add Printer Wizard" appears, select "next".

d. When "Local or Network Printer" in "Add Printer Wizard" appears, select
   "Local printer attached to this computer", check "Automatically detect and
   install my Plug & Play printer", and select "next".

e. "Found New Hardware Wizard" will appear on the screen.  Insert the printer
   driver disk, select "Install from a list or specific location (Advanced)",
   and select "next".

f. When "Please choose your search and installation options" appears, select
   "Search for the best driver in these locations.", un-check "Search removable
   media (floppy,CD-ROM...)", and only check "Include this location in the
   search".  Enter "D:\Drivers\DL7400\English\Win2kxp" and select "next".
   NOTE: The CD drive above is assumed to be D:, make changes if necessary.

g. File copy start.

m. When the screen "Hardware Installation" appears, select "Continue Anyway".
   NOTE: As in 3.1, this is the case when the "Driver Signing" is set to
         "Warn".

i. When "Completing the Found New Hardware Wizard" appears, make sure the
   message "The wizard has installing the software for : FUJITSU DL7400"
   appears, and select "Finish".

j. When "New Printer Detection" appears on the screen, Make sure the message
   "Do you want to print a test page?" appears.
   Select "Yes" or "No", and select "next".

k. When "Add Printer Wizard" appears on the screen, make sure the message
   "Completing the Add Printer Wizard" appears. Select "Finish".

l. The files are copied and the installation for the driver is now completed.
   In [j.], when "Print Test Page" is selected, a dialogue box to inform the
   printing complete will appear when printing is completed.  click the "Yes"
   or "Troubleshoot..." button.
   Note  with Test Page:
     - Printing will proceed based on the printer driver settings at the time.
     - The default values of the page-feeding method is "automatically select"
       with paper size set and "Letter", therefore please prepare Letter paper
       for the test page.
     - Change the setting when using a different size of paper for the test
       page.

m. When installation is complete, an icon of the added printer will appear in
   the "Printers and Faxes" folder.

Printer driver setup is now complete.


3.3.2.2 for WindowsXP Home Edition
==================================
Start Add-printer wizard.
The following is the setup procedure after WindowsXP Home Edition is started
up.
NOTE: Turn on the printer.

a. Go to "Start" -> "Control Panel" -> "Printer and other hardware".

b. Select "Add Printer" from the "Printer and other hardware" screen.

c. When the "Add Printer Wizard" screen appears, select "next".

d. When "Local or Network Printer" in "Add Printer Wizard" appears, select
   "Local printer attached to this computer", check "Automatically detect and
   install my Plug & Play printer", and select "next".

e. For the rest of the procedure, please refer to procedure [e.] and thereafter
   in "3.3.2.1 for WindowsXP Professional".

f. After installation, an icon of the added printer will appear in the
   "Printers and Faxes" folder.

Printer driver setup is now complete.


+++++++++++++++++++++++
3.3.3 Using Plug & Play
+++++++++++++++++++++++
NOTE: Turn off both the PC and the printer.

a. Make sure the printer is connected to the PC, and turn on the printer.

b. Make sure the printer is on-line, turn on the PC, and start WindowsXP.

c. "Welcome to the Found New Hardware Wizard" will appear on the screen.
   Insert the printer driver disk, select "Install from a list or specific
   location (Advanced)", and select "next".

d. When "Please choose your search and installation options" appears, select
   "Search for the best driver in these locations.", un-check "Search removable
   media (floppy,CD-ROM...)", and only check "Include this location in the
   search".  Enter "D:\Drivers\DL7400\English\Win2kxp" and select "next".
   NOTE: The CD drive above is assumed to be D:, make changes if necessary.

e. When the screen "Hardware Installation" appears, select "Continue Anyway".
   NOTE: As in 3.1, this is the case when the "Driver Signing" is set to
         "Warn".

f. File copy start.

g. When "Completing the Found New Hardware Wizard" appears, make sure the
   message "The wizard has installing the software for : FUJITSU DL7400"
   appears, and select "Finish".

Printer driver setup is now complete.



4. Uninstalling the printer driver

-------------------
4.1 for Windows2000
-------------------
Printer driver uninstallation is as follows.

a. Go to "Start" -> "Settings" -> "Printers".

b. Select "FUJITSU DL7400" from the "printers" folder, and select "Delete" from
   the "File" menu.

c. When "Are you sure want to delete the printer 'FUJITSU DL7400'?" appears on
   the screen, select "yes".
   NOTE: If the printer driver is not installed, "Warning: The default printer
         has beeb deleted.  There are printers set up on your computer." will
         appear.  Press the "OK" button.
         If there is no default printer, the message "Warning: The default
         printer has been deleted. The new printer is 'XXXXXX XXXXXXX'
         ('XXXXX XXXXXX' being the newly installed printer) will appear on
         the screen.  Press the "OK" button.

d. Select "Server Properties" from the "File" menu, click on the "Drivers" tab.

e. Select "FUJITSU DL7400" from the "Installed printer drivers:" list, and
   select "Remove".

f. When "Deleting this driver will remove it from the system. Are you sure you
   want to delete FUJITSU DL7400?" appears on the screen, select "Yes".

g. After the drive is deleted, click on "Close" and terminate the "Print server
   properties" dialogue.

h. Turn off the printer and restart the computer.

Printer driver is now removed.


------------------------------
4.2 for WindowsXP Professional
------------------------------
Printer driver uninstallation is as follows.

a. Go to "Start" -> "Control Panel" -> "Printer and other hardware" ->
   "Printers and Faxes".

b. Select "FUJITSU DL7400" from the "Printers and Faxes" folder, and select
   "Delete" from the "File" menu.

c. For the rest of the procedure, please refer to procedure [c.] and thereafter
   in "4.1 for Windows 2000".

Printer driver is now removed.


------------------------------
4.3 for WindowsXP Home Edition
------------------------------
Printer driver uninstallation is as follows.

a. Go to "Start" -> "Control Panel" -> "Printer and other hardware" ->
   "Printers and Faxes".

b. Select "FUJITSU DL7400" from the "Printers and Faxes" folder, and select
   "Delete" from the "File" menu.

c. For the rest of the procedure, please refer to procedure [c.] and thereafter
   in "4.1 for Windows 2000".

Printer driver is now removed.



5. Printer driver setup method

- Document properties such as paper size and others can be set in the "printer
  properties" menu in the application software.

- Depending on the application software used, the paper size settings of the
  application software may be the default rather than that of the "page
  setting" tab.

- The following is the method for each paper feeding (to set such as paper size
  assignment):
  [for Windows2000]
     Go to "Start" -> "Settings" -> "Printers" -> "FUJITSU DL7400", and click
     on the right button of the mouse, select "properties",
     specify the "Form to Tray assignment" from the "Device Settings" tab.

  [for WindowsXP Professional/Home Edition]
      Select "Start" -> "Control Panel" -> "Printer and other hardware" ->
      "Printers and Faxes" -> "FUJITSU DL7400", and click
      on the right button of the mouse, select "properties", specify the "Form
      to Tray assignment" from the "Device Settings" tab.

  NOTE:
  - This method is valid only when the Paper Source setting of the printer
    driver is set at the "Automatically Select".
  - Please make sure the actual paper size matches the selected paper size.
    Use the "Manual Paper Feed" the actual paper size differs from the selected
    paper size.

- Refer read the chapter of software in the user's manual for further details.



6. Others

a. The emulation for this driver is in the "DPL24C+" mode.
   Make sure the setting of the printer installation corresponds to it.

b. Users are required to adjust devices for such as the paper insertion.
   Please make sure the paper settings, as well as the settings from the
   operation panel correspond to the printer.

c. Printing from Windows95 application software under the Windows2000 or
   WindowsXP environments may give different results.

d. The contents of "Properties" of the printer driver and "Printing
   Preferences" of the printer may overlap.  Please make necessary adjustments
   to avoid any possible malfunction.

e. Some specified printer fonts from the application may not be used depending
   on the data format.

f. Paper size from the "Server Properties" can be set to a maximum width of
   15 inches.  Adjust the right and left margins not the exceed an 13.6 inch
   paper width as the data may not be properly printed.

   The paper length can be set starting from 1inch (about 25.4 mm).
   However, when specifying any of the paper feed ports below, do not specify
   paper 2.76 inches (about 70.0 mm) or less in length.
   Otherwise, the paper will not be properly fed, leading to a paper jam.

   - manual feed
   - CSF #1
   - CSF #2

g. When printing with a "Page per Sheet" specification from the "layout" tab in
   the print menu, frame lines may not be printed with some applications.

h. Based on the application, zoom-in/out printing may always result in
   10.5-size fonts.

i. Paper with a length of 3 inches - 14 inches isruled with a width of 15
   inches.
   When using paper with a width less than 15 inches, please make adjustments
   to the right margin of the application not to exceed the maximum possible
   range.

j. When using Continuous form with a tractor feeder on this printer, the
   possible folding length is 4 inches or more.
   When the folding length is the same as the page length, use paper with a
   folding length of more than 4 inches.

k. If printing is cancelled from the printer port during printing, restart the
   printer.
   Continuing printing without restarting the printer may result in problems
   such as garbled texts.

l. Continuous Form
   - Both the upper and lower margins for continuous form are set at 0mm in
     this printer driver.  It is recommended that the upper and lower margins
     for continuous form using Tractor feeder with this printer is more than
     25.4mm
   - The printing head and the ribbon may be damaged when printing on the
     perforation lines and sprocket holes.

m. Envelopes
   - Print only on the surface side.  Do not print on the flap side as the
     envelope may be jammed.
   - Do not print on envelopes with a window or double-layered envelopes.
   - Printing outside the margin out of guarantee.
   - Refer to the following for paper-feeding directions to avoid a paper jam.
          +---------------------------------------------------------+
          |*                                                       *|
          | *                                                     * |
          |  *          insert paper in this direction           *  |
          |   *                                                 *   |
          |    * * * * * * * * * * * * * * * * * * * * * * * * *    |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |                            |                            |
          |  * * * * * * * * * * * * * * * * * * * * * * * * * * *  |
          | *                                                     * |
          |*                                                       *|
          +---------------------------------------------------------+

n. Adjust the paper guide when printing on A3 Rotated paper.
   (The left printing margin is set at 38mm)

o. Under Windows 2000, connect DL7400 to your PC before installing Printer
   Driver, the following message appears as "Unknown Device", "New Hardware
   Detection Wizard" will start.
   Install DL7400 Printer Driver according to this Wizard, or after clicking
   "Cancel" install DL7400 Printer Driver in "Addition of new Printer" in
   Printer Folder.

p. The DL7400 printer driver to every connecting port will be set if the
   connecting USB port is changed.  (e.g. FUJITSU dl7400 (copy 2) etc.)
   Since every setting of the printer driver is the initial value, so
   change the setting according to the using state.

q. When Printer Font is specified and print it, change Language setting
   to WCP1252 by DLMENU or Offline Setup.
   Otherwise, print result may not be correct.

r. Note for sharing printer into Network environment
    -Printer shared by Network environment may not be able to be used with
     Windows XP SP2 because of Windows Firewall.
     In this case, change the exceptional settings of Windows Firewall with
     following procedure.
     1.Select "Start"->"Control Panel"->"Security Center".
     2.Select "Windows Firewall".
     3.When the dialogo box of "Windows Firewall", select "Exceptions".
     4.Check "File and Printer Sharing", and click "OK".

      **In case that the printer installed into Windows XP SP2 is set
      with Network sharing setting, automatically checked to "File and
      printer share".

s. Regarding the DL7400 Printer
   Ejecting cut sheet paper to the cut sheet table in front sometimes leads to
   wait for removal of a cut sheet (blinking lamp for ejection in front).
   In such cases, remove the paper from the cut sheet table, load the next
   paper, and then press the online switch.

   **The error message displayed when status of wait for removal of a cut
   sheet (blinking lamp for ejection in front) occurs during printing 
   indicates a time out error, not a paper out error.

t. Changing the paper feed port or paper size with the page setting or
   document setting in the application.
   The margin size outside the print enabled area can be set even when the
   printer driver specified value is not correctly reflected.
   To prevent this, first set the paper feed port and paper size you intend to
   use with printer properties in the printer folder.  Then change the paper
   feed port and paper size in the application, or avoid setting the margin
   size outside the print enabled area.  For information on the print enabled
   area (minimal margin size) per individual paper feed ports and paper sizes,
   refer to the Users Manual.

- About the trademark
    Company names and product names mentioned above are registered trademarks
    or trademarks of each company.

[End]
